#!/bin/sh
DRIVERS=/sbin
RESCUE=/boot/rescue

if [ "$1" != start ]
then	exit
fi

service up $DRIVERS/rescue -dev /dev/rescue -args 128 -period 4HZ
mkfs /dev/rescue || exit
mount /dev/rescue $RESCUE || exit
label=`sysenv label`
case "$label" in
AT)
	d=at_wini
	;;
FLOPPY)
	d=floppy
	;;
BIOS)
	d=bios_wini
	;;
*)	exit
	;;
esac
cp $DRIVERS/$d $RESCUE/driver
service rescue $RESCUE 
